#### STICHTING BAKENS VERZET

#### 1018 AM AMSTERDAM, THE NETHERLANDS

Director,

T.E.(Terry) Manning,

Schoener 50,

1771 ED Wieringerwerf,

The Netherlands.

Tel: 0031-227-604128

Homepage: http://www.flowman.nl

E-mail: (nameatendofline)@xs4all.nl : bakensverzet

## MODEL FOR SUSTAINABLE SELF-FINANCING INTEGRATED RURAL AND POOR URBAN DEVELOPMENT FOR THE WORLD'S POOR

Incorporating innovative social, financial, economic, local administrative and productive structures, numerous renewable energy applications, with an important role for women in poverty alleviation in rural and poor urban environments.

"Money is not the key that opens the gates of the market but the bolt that bars them"

Gesell, Silvio The Natural Economic Order

Revised English edition, Peter Owen, London 1958, page 228

Edition 14: 31 October, 2007

(EN FRANÇAIS)

## 6.29 Drinking water structures.

The distributed drinking water supply structures are the structures which need the largest formal money capital investments. They will defined by the people themselves during a capacitation workshop following the formation of most of the other structures planned. The following general indications are therefore subject to changes, some of them important, from one project application to another. The following information should, however, give a fair idea of the size and nature of project applications.

See drawings:

PROJECT STRUCTURES
TANK COMMISSIONS – THE KEY STRUCTURES
WELL COMMISSIONS
DRAWING OF DRINKING WATER SUPPLY STRUCTURES
DRAWING OF A DRINKING WATER TANK INSTALLATION AREA

DRAWING OF COMPLETE WASTE RECYCLING STRUCTURE

### 00.0.00.0. Water supply summary (example)

###### Villages | ##### Inhabitants | Liters/day | Boreholes/wells | Handpumps | Solar pumps | Watts installed
Villages du canton de Sedomi | 27071 | 0781 | 19 | 057 | 120 | 036000
Villages du canton de Gboto | 20424 | 0515 | 13 | 039 | 069 | 020700
Total | 47495 | 1296 | 32 | 96 | 189 | 56700

Basic information for drinking water supply (example):

Inhabitants : 47495
Boreholes : 32
Approximately litres/day 1.296.000 (1296 m3)
Solar pumps installed : 189
Installed photovoltaic power : 56.7 KW
15 m3 water tanks :189
Back-up hand pumps : 96 being 32 triple sets.
Pipelines from boreholes to water tanks (estimation) : 200000m.

Principles applied for placing drinking water structures
Boreholes and wells and their equipment
Water points near family homes
Some budget items applicable to the water supply structures

List of files connected to hygiene education, water and sanitation.

Forward : The third phase of project execution.

Back : The local radio station.

Menu group 6 work files : The phases of project execution.

Main menu for the project work file groups.

Main index of the project work files.

Homepage of the Model.

Bakens Verzet Homepage.